display_name = "Sega MS/GG/MD/CD/32X (Picodrive)"
authors = "notaz|fdave"
supported_extensions = "md|smd|gen|sms|gg|sg|bin|cue|ios|32x"
corename = "Picodrive"
manufacturer = "Sega"
systemname = "Sega 16bit + 32X (Various)"
license = "MAME"
permissions = "dynarec_optional"
firmware_count = 3
firmware0_desc = "bios_CD_E.bin (MegaCD EU BIOS)"
firmware0_path = "bios_CD_E.bin"
firmware0_opt = "false"
firmware1_desc = "bios_CD_U.bin (SegaCD US BIOS)"
firmware1_path = "bios_CD_U.bin"
firmware1_opt = "false"
firmware2_desc = "bios_CD_J.bin (MegaCD JP BIOS)"
firmware2_path = "bios_CD_J.bin"
firmware2_opt = "false"
